IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2024-06-19T10:03:57"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.90.15 - Exporter 21.1.90.15 - Alternate UI 19.3.0.0"
Application: "Autodesk Revit 2021 (ENG)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENG)"

People and organizations
  Person "PiotrBocian.com" of Organization (no name given)
  Owner history of Person "PiotrBocian.com" of Organization (no name given) | application "Autodesk Revit 2021 (ENG)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENG)" | change NOCHANGE | created 1718787603 (2024-06-19T09:00:03Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:Circle Head - Project Datum" | elevation 0.
        contains 2 elements
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW214" | object type "Floor:NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW214" | FLOORING | names: "Floor:NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW214:221799" | material: layers "Floor:NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW214" ("NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW214" 26.) | property sets: IFC, COBie, BOS_General, NBS_Data
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW215Gripdeck" | object type "Floor:NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW215Gripdeck" | FLOORING | names: "Floor:NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW215Gripdeck:221946" | material: layers "Floor:NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW215Gripdeck" ("NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW215Gripdeck" 26.) | property sets: IFC, COBie, BOS_General, NBS_Data

Types
  IFCCOVERINGTYPE "Floor:NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW214" | FLOORING | 1 occurrence | material: layers "Floor:NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW214" ("NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW214" 26.) | property sets: IFC, COBie, BOS_General, NBS_Data
  IFCCOVERINGTYPE "Floor:NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW215Gripdeck" | FLOORING | 1 occurrence | material: layers "Floor:NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW215Gripdeck" ("NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW215Gripdeck" 26.) | property sets: IFC, COBie, BOS_General, NBS_Data

Property sets
  COBie | properties | on 3 objects (1 IFCBUILDING, 1 IFCPROJECT, 1 IFCSITE)
    Category = "Project Information" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_71_97_78:Softwood deck boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Thermally modified Scandinavian Scots Pine external decking." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Brushed,Smooth,Other" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "mail@russwood.co.uk" (IFCTEXT)
    Material = "Timber" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Thermopine® Decking RW214" (IFCTEXT)
    Name = "SoftwoodDeckBoards_ThermopineDecking_RW214_RusswoodLtd" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_71_97_78:Softwood deck boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Thermally modified Scandinavian Scots Pine external decking." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Brushed,Smooth,Other" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "mail@russwood.co.uk" (IFCTEXT)
    Material = "Timber" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Thermopine® Decking RW215 Gripdeck" (IFCTEXT)
    Name = "SoftwoodDeckBoards_ThermopineDecking_RW215Gripdeck_RusswoodLtd" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCTEXT)
    Name = "Level 0" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_97_78:Softwood deck boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Thermally modified Scandinavian Scots Pine external decking." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Brushed,Smooth,Other" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "mail@russwood.co.uk" (IFCTEXT)
    Material = "Timber" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Thermopine® Decking RW214" (IFCTEXT)
    Name = "SoftwoodDeckBoards_ThermopineDecking_RW214_RusswoodLtd" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_97_78:Softwood deck boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Thermally modified Scandinavian Scots Pine external decking." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Brushed,Smooth,Other" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "mail@russwood.co.uk" (IFCTEXT)
    Material = "Timber" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Thermopine® Decking RW215 Gripdeck" (IFCTEXT)
    Name = "SoftwoodDeckBoards_ThermopineDecking_RW215Gripdeck_RusswoodLtd" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 3 objects (1 IFCBUILDING, 1 IFCPROJECT, 1 IFCSITE)
    Author (no value)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW214" (IFCTEXT)
    ManufacturerName = "Russwood Ltd" (IFCTEXT)
    ManufacturerURL = "www.russwood.co.uk" (IFCTEXT)
    NBSInstanceId = "8838e3b4-14b3-45d8-a7dc-b20e8f4cb612" (IFCTEXT)
    NBSObjectId = "e4e1cc5c-182e-41f3-a75a-edbf855e8a09" (IFCTEXT)
    NBSVariantId = "1f9dd891-6fb0-486a-3e7d-9f8050436f01" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/e4e1cc5c-182e-41f3-a75a-edbf855e8a09/8838e3b4-14b3-45d8-a7dc-b20e8f4cb612" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_97_78" (IFCTEXT)
    Uniclass2015Title = "Softwood deck boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.34" (IFCTEXT)
    Version = "3" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_RusswoodLtd_SoftwoodDeckBoards_ThermopineDecking_RW215Gripdeck" (IFCTEXT)
    ManufacturerName = "Russwood Ltd" (IFCTEXT)
    ManufacturerURL = "www.russwood.co.uk" (IFCTEXT)
    NBSInstanceId = "8838e3b4-14b3-45d8-a7dc-b20e8f4cb612" (IFCTEXT)
    NBSObjectId = "e4e1cc5c-182e-41f3-a75a-edbf855e8a09" (IFCTEXT)
    NBSVariantId = "087f164b-7e76-03e0-9013-5e6d715afc74" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/e4e1cc5c-182e-41f3-a75a-edbf855e8a09/8838e3b4-14b3-45d8-a7dc-b20e8f4cb612" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_97_78" (IFCTEXT)
    Uniclass2015Title = "Softwood deck boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.34" (IFCTEXT)
    Version = "3" (IFCTEXT)
  IFC | properties | on 2 objects (2 IFCCOVERING) | on 2 type objects
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "FLOORING" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    CountryOfMaterialOrigin = "Finland" (IFCTEXT)
    CountryOfProductManufacture = "Finland" (IFCTEXT)
    Density = "420 kg/m³" (IFCTEXT)
    EmbodiedCarbon = "770" (IFCTEXT)
    FinishAsDeliveredFlame-retardantTreatment = "Manufacturer's standard" (IFCTEXT)
    FinishedSizeSection = "115 x 26 mm" (IFCTEXT)
    Fixings = "SenoFix® FT,L-GoFix® MS A2 stainless-steel screws and KompeFix®" (IFCTEXT)
    MoistureContentValue = "6–8%" (IFCTEXT)
    Profile = "RW214" (IFCTEXT)
    Recyclability = "Yes" (IFCTEXT)
    Species = "Scots pine" (IFCTEXT)
    SurfaceFinish = "Brushed,Planed" (IFCTEXT)
    Third-partyCertification = "PEFC certified" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    CountryOfMaterialOrigin = "Finland" (IFCTEXT)
    CountryOfProductManufacture = "Finland" (IFCTEXT)
    Density = "420 kg/m³" (IFCTEXT)
    EmbodiedCarbon = "770" (IFCTEXT)
    FinishAsDeliveredFlame-retardantTreatment = "Manufacturer's standard" (IFCTEXT)
    FinishedSizeSection = "115 x 26 mm" (IFCTEXT)
    Fixings = "SenoFix® FT,L-GoFix® MS A2 stainless-steel screws and KompeFix®" (IFCTEXT)
    MoistureContentValue = "6–8%" (IFCTEXT)
    Profile = "RW215" (IFCTEXT)
    Recyclability = "Yes" (IFCTEXT)
    Species = "Scots pine" (IFCTEXT)
    SurfaceFinish = "Gripdeck" (IFCTEXT)
    Third-partyCertification = "PEFC certified" (IFCTEXT)