IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2024-06-19T09:56:14"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.90.15 - Exporter 21.1.90.15 - Alternate UI 19.3.0.0"
Application: "Autodesk Revit 2021 (ENG)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENG)"

People and organizations
  Person "PiotrBocian.com" of Organization (no name given)
  Owner history of Person "PiotrBocian.com" of Organization (no name given) | application "Autodesk Revit 2021 (ENG)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENG)" | change NOCHANGE | created 1718787238 (2024-06-19T08:53:58Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:Circle Head - Project Datum" | elevation 0.
        contains 1 element
          1 x IFCCOVERING | type IFCCOVERINGTYPE "Floor:NBS_RusswoodLtd_SoftwoodStrips_DouglasFirFlooring" | object type "Floor:NBS_RusswoodLtd_SoftwoodStrips_DouglasFirFlooring" | FLOORING | names: "Floor:NBS_RusswoodLtd_SoftwoodStrips_DouglasFirFlooring:221809" | material: layers "Floor:NBS_RusswoodLtd_SoftwoodStrips_DouglasFirFlooring" ("NBS_RusswoodLtd_SoftwoodStrips_DouglasFirFlooring" 17.) | property sets: IFC, COBie, BOS_General, NBS_Data

Types
  IFCCOVERINGTYPE "Floor:NBS_RusswoodLtd_SoftwoodStrips_DouglasFirFlooring" | FLOORING | 1 occurrence | material: layers "Floor:NBS_RusswoodLtd_SoftwoodStrips_DouglasFirFlooring" ("NBS_RusswoodLtd_SoftwoodStrips_DouglasFirFlooring" 17.) | property sets: IFC, COBie, BOS_General, NBS_Data

Property sets
  COBie | properties | on 3 objects (1 IFCBUILDING, 1 IFCPROJECT, 1 IFCSITE)
    Category = "Project Information" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_25_71_97_83:Softwood strips" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Engineered Douglas Fir flooring." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Oiled" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "mail@russwood.co.uk" (IFCTEXT)
    Material = "Wood" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Douglas Fir Flooring" (IFCTEXT)
    Name = "SoftwoodStrips_DouglasFirFlooring_RusswoodLtd" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCTEXT)
    Name = "Level 0" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_97_83:Softwood strips" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Engineered Douglas Fir flooring." (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Oiled" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "mail@russwood.co.uk" (IFCTEXT)
    Material = "Wood" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "Douglas Fir Flooring" (IFCTEXT)
    Name = "SoftwoodStrips_DouglasFirFlooring_RusswoodLtd" (IFCTEXT)
    NominalHeight = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 3 objects (1 IFCBUILDING, 1 IFCPROJECT, 1 IFCSITE)
    Author (no value)
  BOS_General | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_RusswoodLtd_SoftwoodStrips_DouglasFirFlooring" (IFCTEXT)
    ManufacturerName = "Russwood Ltd" (IFCTEXT)
    ManufacturerURL = "www.russwood.co.uk" (IFCTEXT)
    NBSInstanceId = "e5d54210-9e6f-402e-a975-8f184df0e9f9" (IFCTEXT)
    NBSObjectId = "7681171e-b75d-4db2-86db-4b101f01d7b4" (IFCTEXT)
    NBSVariantId = "00000000-0000-0000-0000-000000000000" (IFCTEXT)
    ProductInformation = "https://source.thenbs.com/product/-/7681171e-b75d-4db2-86db-4b101f01d7b4/e5d54210-9e6f-402e-a975-8f184df0e9f9" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_97_83" (IFCTEXT)
    Uniclass2015Title = "Softwood strips" (IFCTEXT)
    Uniclass2015Version = "Products v1.34" (IFCTEXT)
    Version = "3" (IFCTEXT)
  IFC | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "FLOORING" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING) | on 1 type object
    Construction = "Three-layer construction, comprising two outer layers of 4 mm Douglas fir and a 9 mm Birch plywood core" (IFCTEXT)
    CountryOfMaterialOrigin = "Europe" (IFCTEXT)
    CountryOfProductManufacture = "Belgium" (IFCTEXT)
    Density = "530 kg/m³" (IFCTEXT)
    DryingMethod = "Kiln-dried" (IFCTEXT)
    Durability = "Class 3" (IFCTEXT)
    Edges = "Tongued-and-grooved" (IFCTEXT)
    FinishAndColour = "Signature White" (IFCTEXT)
    FinishAsDeliveredAppliedFinish = "Hardwax oil" (IFCTEXT)
    FinishedSizeFaceWidth = "350 mm" (IFCTEXT)
    FinishedSizeThickness = "17 mm" (IFCTEXT)
    JankaRating = "660 lb (2940 N)" (IFCTEXT)
    ReactionToFireClassification = "To EN 14342, Cfl-S1" (IFCTEXT)
    SoftwoodMoistureContent = "6–8%" (IFCTEXT)
    Species = "Douglas fir" (IFCTEXT)
    Standard = "To EN 14342 and BS EN 13489" (IFCTEXT)
    Third-partyCertification = "FSC® and PEFC certified" (IFCTEXT)
    VolatileOrganicCompoundsVOCEmissionsLevelMaximum = "Class E1 (<0.124 mg/m³)" (IFCTEXT)